C4BG0UF1 - 206 CABRIOLET

REMOVAL - REFITTING BOOT UPPER COVER

1 - REMOVAL

Change the vehicle into the coupé version .

REMOVE THE BOOT COVER TRIM .

Fold up the tray (luggage cover screen) .

IMMOBILISE THE BOOT COVER .

Remove the striker fixings (1) .

Detach the harness (2) and only the (3) cables from the mounting clips .

Detach the clamps (4) from the harness .

Disconnect the connector (5) .

Remove the fixings (6) and support the boot ; Two operators are necessary .

Remove the boot upper cover .

2 - REFITTING

Proceed in the reverse order to removal .

ADJUST THE CLEARANCES AND FLUSH FITTING .

ADJUST THE BOOT UPPER COVER LOCKING MECHANISM .

Tighten :

- fasteners (1) : 1 ± 0.1 da.Nm
- fasteners (6) : 2.3 ± 0.30 da.Nm

Test operation .