C7AP0KV1 - 206

FITTING SPECIAL ALARM

1 - PRESENTATION

(1) Compact unit or siren .

(2) Alarm unit (modular system) .

(3) Display LED .

(4) Ultrasonic sensor .

(5) Luggage compartment switch .

(6) Built-in systems interface connection harness/Alarm .

(7) Bonnet switch .

2 - MODULAR ALARM PART NO. 9671.X3/9671.Z3

2 - 1 - COMPOSITION

description | reference | quantity
--- | --- | ---
siren | 1 | 1
alarm unit (modular system) | 2 | 1
display LED | 3 | 1
ultrasonic sensor (according to model) | 4 | 2
luggage compartment switch Part No. 8724.74 | 5 | 1
built-in systems interface connection harness/alarm | 6 | 1
bonnet switch | 7 | 1
siren harness | 8 | 1
siren mounting plate | 9 | 1
sleeve (wire feed) | 10 | 1
wire : red | 11 | 1
wire : white/green | 12 | 1
siren harness liaison connector | 13 | 1
26-way connector : mauve | 14 | 1
26-way connector : blue | 15 | 1
16-way connector : black (caliper) | 16 | 1
16-way connector : black | 17 | 1
alarm unit connector | 18 | 1
LED liaison connector | 19 | 1
LED connector | 20 | 1
siren liaison connector | 21 | 1
siren harness connector | 22 | 1
terminals | 23 | 5
bonnet switch liaison connector | 24 | 1
bonnet switch connector | 25 | 1
luggage compartment switch harness | 26 | 1
mastic | 27 | 1
fuse | 28 | 1

3 - COMPACT ALARM PART NO. 9671.Z5

3 - 1 - COMPOSITION

description | reference | quantity
--- | --- | ---
compact alarm | 1 | 1
display LED | 3 | 1
ultrasonic sensor | 4 | 2
luggage compartment switch Part No. 8724.74 | 5 | 1
built-in systems interface connection harness/alarm | 6 | 1
bonnet switch | 7 | 1
siren harness | 8 | 1
siren mounting plate | 9 | 1
sleeve (wire feed) | 10 | 1
wire : red | 11 | 1
wire : blue | 12 | 1
siren harness liaison connector | 13 | 1
26-way connector : mauve | 14 | 1
26-way connector : blue | 15 | 1
16-way connector : black (caliper) | 16 | 1
16-way connector : black | 17 | 1
LED liaison connector | 19 | 1
LED connector | 20 | 1
siren liaison connector | 21 | 1
siren harness connector | 22 | 1
bonnet switch liaison connector | 24 | 1
bonnet switch connector | 25 | 1
luggage compartment switch harness | 26 | 1
mastic | 27 | 1
fuse | 28 | 1
mounting cover | 31 | 1

4 - FITTING

4 - 1 - VEHICLE PREPARATION

Open the bonnet .

Disconnect the battery + terminal .

Remove :

- the flap (32)
- the switch bracket (33)

Remove :

- the bolt (34)
- the Built-in Systems Interface (35)
- the bolts (36)
- the passenger compartment fuse box (37)

Remove : The rubber blank (38) .

Using a screwdriver, drive out the plastic protective cover from the bottom of the recess to free the bulkhead opening .

4 - 2 - FITTING : SIREN (1)/BONNET SWITCH (7)

To the siren harness (8) , fit the grommet (10) at 400 mm from the siren liaison connector (21) .

Seal using the mastic (27) which is to be used like modelling clay .

Remove :

- the inertia switch (39)
- the bracket and the air conditioning thermostat (40) (according to specification)

Pass the siren harness (8) fitted with the grommet (10) into the bulkhead opening .

Remove the grille .

Route the bonnet switch liaison connector wire (24) along the original harness as far as the left-hand direction indicator and clip it .

Clip the bonnet switch (7) .

Clip the wire to the bonnet opening cable (41) .

Connect the connector (24) to the connector (25) .

Passenger compartment side :

- fit the terminals (23) (according to model) and the connector (22) onto the siren harness (8) so that the colours of the wires match at connector (13) of the BSI/alarm connection harness

AIR CONDITIONING

Fit the siren securing plate (9) to the welded bolt on the shock absorber turret .

Connect the connector (21) for the siren harness (8) to the siren (1) .

Compact alarm :

- secure the cover (31) to the siren (1) using the 4 black bolts

Secure the siren (1) to the plate (9) .

Position the air conditioning thermostat bracket (40) .

Connect the connector (21) for the siren harness (8) to the siren (1) .

Compact alarm :

- secure the cover (31) to the siren (1) using the 4 black bolts

Secure the siren to the bracket (40) then secure the bracket (40) .

ALL MODELS

4 - 3 - FITTING : BUILT-IN SYSTEMS INTERFACE CONNECTION HARNESS/(6) ALARM

Disconnect the blue connector (42) and connect it to the purple connector (14) for the BSI/alarm harness (6) .

Disconnect the black connector (43) and connect it to the black connector (17) for the BSI/alarm harness (6) .

Connect the BSI/alarm harness connectors (15) and (16) to the BSI .

Clip the BSI/alarm harness (6) along the original harness .

Unclip the passenger compartment fuse box double lock (52) .

Clip the terminal of the red wire (11) of the BSI/alarm harness (6) to the passenger compartment fuse box (37) at terminal A10 (44) .

Insert the fuse (28) (15 A) in position 10 .

Connect the connector (22) for the siren harness (8) to the BSI/alarm harness connector (13) .

4 - 4 - FITTING : DISPLAY LED (3)

Unclip the upper centre panel (45) .

Route the LED connection connector wire (19) for the BSI/alarm harness (6) along the original harnesses as far as the clock .

Connect the connector (19) to the connector (20) for the display LED (3) .

Make a hole in the centre of the upper centre panel (45), diameter 8 mm .

Fit the display LED (3) .

4 - 5 - FITTING : ULTRASONIC SENSOR (4) (ACCORDING TO MODEL)

Unclip the left and right hand windscreen pillars .

Position the ultrasonic sensors (4) at the top of the windscreen pillars .

Route the wire of the right-hand sensor under the headlining retaining it with the mastic (27) at regular intervals .

Route the wires of the sensors along the windscreen pillar to the passenger compartment fuse box .

Compact alarm :

- connect the ultrasonic sensors to the siren harness (8)

4 - 6 - FITTING : LUGGAGE COMPARTMENT SWITCH (5)

Remove the luggage compartment carpet (47) (Partly) (left side) .

Remove the luggage compartment side trim (46) (left side) .

Mark the position of the striker (Tailgate) .

Remove the striker .

Fit the tailgate striker part number 8724.74 fitted with the luggage compartment switch (5) .

Connect the luggage compartment switch harness connector (26) to the striker (5) .

Secure the luggage compartment switch harness earth terminal (26) to the striker right-hand mounting bolt (48) .

Clip the harness (26) using two fasteners (30) part number 6995.45 and route it in the sheathing (49) as far as the rear seat cushion .

Route the luggage compartment switch harness wire (26) along the original harness .

Connect the white/green wire or blue wire (12) of the BSI/alarm harness (6) to the luggage compartment switch harness wire (26) using a RAYCHEM sleeve (50) (according to model) .

4 - 7 - FITTING : REAR DOOR CONTACT (VEHICLE WITHOUT CENTRAL LOCKING)

Remove the B/C post lower trims (On both sides) .

Drill a 12 mm diameter hole in the centre pillars observing the dimensions .

Fit the door sill switches part number 6366.78 and mark the position of the securing holes .

Drill the securing holes to a diameter of 3 mm .

Protect the holes with anti-corrosion product .

Make the connections to the switches using clips part number 6542.56 .

Connect the switches to the luggage compartment switch harness wire (26) using a RAYCHEM sleeve .

Secure the switches using the bolts part number 6924.34 .

4 - 8 - FITTING : ALARM UNIT (ACCORDING TO MODEL)

Connect the connector (18) for the BSI/alarm harness (6) to the unit (2) .

Remove the security card from the unit so that it can be given to the customer (according to model) .

Connect the ultrasonic sensors to the unit (according to model) .

Secure the unit (2) to the left-hand ventilation hose (51) using the plastic clip (29) .

(Notice valid subject to product modification) .