B2FM00K1 - 206

USE LIGAREX CLIPS

1 - SPECIAL TOOLS

[1] Clips-bindings fitting kit .

2 - OPERATION

Pull the metal strip through the loop and fold it back approximately 2 cm (A) .

Pull out a length of metal strip equal to 2 turns of the part to be bound plus 6 cm .

Cut the metal strip .

Pass the metal strip in the loop around twice, with the round hole towards you .

Fold the strip back slightly to prevent it from slipping .

Open the clamp .

Engage the strip in the narrowest slit, one to two cm above the loop .

Place the nose of the pliers in the loop hole .

Tighten the metal strip by closing the pliers .

NOTE : if the strip is not tightened enough, repeat the operation .

Fold back the pliers allowing the handles to partially open .

Detach the pliers to the side .

Cut the metal strip using the pliers 15 mm from the loop .

Support the strip with the loop using the pliers (B) .

Fold back the metal strip under the loop using another pair of pliers .

Flatten the loop using a mallet .