C5CB02F1 - 206

IDENTIFICATION BONDING KIT GLASS

[1] Twin-component ultra-rapid setting kit (Part No. 9799.58) :

- 1 set(s) of 450 ml cartridges + mixer
- 1 primer(s) for glass 15 ml (green)
- 1 primer for sheet metal 15 ml (red)
- 1 bottle of degreasing agent (Bétawipe) 15 ml (yellow)
- 2 applicator pad(s)
- 2 nozzles

[2] Monocomponent rapid setting kit (Part No. 9799.96) :

- 1 cartridge 300 ml
- 1 primer(s) for glass 15 ml (green)
- 1 primer for sheet metal 15 ml (red)
- 1 bottle of degreasing agent (Bétawipe) 15 ml (yellow)
- 2 primer application pads
- 2 nozzles

procedure GURIT
| Part No. | drying time
--- | --- | ---
| kit(s) | additional cartridge | vehicle without airbag | vehicle with airbag
ultra-rapid setting | 9799.58 | - | 0,50 h | 2,00 h (at 23 °C)
rapid setting | 9799.96 | 9725.21 | 1,50 h | 8,00 h

[3] Kit(s) (Monocomponent) :

- 1 cartridge 310 ml
- 1 glass/metal primer 15 ml
- 1 bottle of degreasing agent 15 ml
- 2 applicator pad(s)
- 4 shims
- cleaning paper
- operating instructions

procedure LOCTITE
| Part No. | drying time
--- | --- | ---
| kit(s) | additional cartridge | vehicle without airbag | vehicle with airbag
ultra-rapid setting (*) | 9799.E3 | 9726.74 | 0,50 h | 0,50 h
rapid setting | 9799.E4 | 9726.75 | 1,50 h | 6,00 h
standard setting | 9799.E5 | 9726.76 | 2,50 h | 12,00 h
(*) USE THE CARTRIDGE HEATER [6]