B1BT0AK1 - 206 DW10TD ENGINE

BLEEDING FUEL SUPPLY SYSTEM

Slacken the bolts (2) .

CONNECT THE FEMALE CONNECTOR Ø 10 MM OF THE TOOL [14] IN THE PLACE OF THE PIPE (3) AT (E) .

DISCONNECT THE FUEL RETURN PIPE (1) AND INSERT THE CONNECTORS Ø 8 MM OF THE TOOL [14] IN THE FUEL RETURN CIRCUIT .

Switch the ignition on and off 10 times in order to fill and bleed the fuel filter .

Remove :

- THE TOOL [14]
- THE TOOL [6] FROM THE PIPE (3)

Couple up the pipes (3) - (1) .

Switch the ignition on and off 2 times .

Tighten the bolt (2) .

Start the engine .

Check there are no leaks .