E5AB1DK1 - 206 DW10TD ENGINE

PRESENTATION TOOLING ENGINE

kit for engine(s) DW
reference | description | reference | reference
--- | --- | --- | ---
[1] | kit | (-).0188-ZX | (-).0188
[1a] | timing side crankshaft seal fitting drift (drift) | (-).0188 - A1 | (-).0188 - A
[1b] | timing side crankshaft seal fitting drift (cone) | (-).0188 - A2 | (-).0188 - A
[1c] | engine flywheel side crankshaft seat fitting drift (cone) | (-).0188 - B1 | (-).0188 - B
[1d] | engine flywheel side crankshaft seat fitting drift (drift) | (-).0188 - B1 | (-).0188 - B
[1e] | camshaft seal fitting drift (cone) | (-).0188 - C1 | (-).0188 - C
[1f] | camshaft seal fitting drift (drift) | (-).0188 -C1 | (-).0188 - C
[1g] | single engine flywheel setting pin | (-).0188 - D | (-).0188 - D
[1h] | bolt(s) M8 x 125 length 45 mm (overhead camshaft setting rod) | (-).0188 - E | (-).0188 - E
[1i] | flywheel stop | (-).0188 - F | (-).0188 - F
[1j] | tensioner roller setting rod | (-).0188 - G | -
[1k] | injection pump setting pin | (-).0188 - H | -
[1l] | tension lever square 8 mm square 7 mm | (-).0188 - J1 (-).0188 - J2 | (-).0188 - J
[1m] | belt retaining clip | (-).0188 - K | -
[1n] | cylinder head releasing levers (quantity 2) | (-).0188 - L | (-).0188 - L
[1p] | camshaft setting rod | (-).0188 - M | -

kit for engine(s) DW (continued)
reference | description | reference | reference
--- | --- | --- | ---
[1] | kit | (-).0188 - ZX | (-).0188
[1q] | camshaft seal fitting drift (drift) (cone) | (-).0188 - N | (-).0188 - N
[1r] | crankshaft pulley extractor | (-).0188 - P | (-).0188 - P
[1s] | dynamic tensioner roller pins (pin ø 4) (pin ø 2) | (-).0188 - Q | (-).0188 - Q
[1t] | kit for detaching the high pressure pump | (-).0188 - R | (-).0188 - R
[1u] | set of plugs | (-).0188 - T | (-).0188 - T
[1v] | compression checking kit | (-).0188 - U | (-).0188 - U
[1w] | pulley immobilisation pin | (-).0188 - V | (-).0188 - V
[1x] | valve stem seal fitting tool | (-).188 - W | (-).0188 - W
[1y] | double engine flywheel setting pin | (-).0188 - X | (-).0188 - X
[1z] | flywheel setting rod | (-).0188 - Y | (-).0188 - Y
[1Aa] | dynamic tensioner compression lever | (-).0188 - Z | (-).0188 - Z

reference | description | reference | reference
--- | --- | --- | ---
[2] | tension measuring equipment | (-).0192 | (-).0192
[3] | angular locking cotter | FACOM D360 type | 4069-T
[4] | cylinder head bolt socket | (-).0185 | FACOM STX 14

reference | description | reference | reference
--- | --- | --- | ---
[5] | pin + dial gauge support | (-).0504 | 5602 - T
[6] | bearing no. 1 side seals fitting tool | (-).0153-A | 7004-T.F
[7] | dial gauge with securing lug | (-).01504 | 2437-T
[8] | dial gauge support rod | (-).0113 - EZ + FZ | 1132-T
[9] | dial gauge carrier

reference | description | reference | reference
--- | --- | --- | ---
[10] | pipe spanner | (-).1603 - | 4220-T.D
[11] | pipe spanner | (-).1603 - G | 4220-T.C

reference | description | reference | reference
--- | --- | --- | ---
[12] | valve lifter cup press | FACOM U43 - LA+ U43 - LA16 - 21 | FACOM U43 - LA+ U43 - LA16 - 21

reference | description | reference | reference
--- | --- | --- | ---
[13] | valve stem oil seal pliers | (-).0170-A | 4517-T (kit 4507-T)

reference | description | reference | reference
--- | --- | --- | ---
[14] | crankshaft spanner | (-).0117-EZ | XXX
[15] | dial gauge support | (-).0110-H | 1754 - T bis

reference | description | reference | reference
--- | --- | --- | ---
[16] | stand | DESVIL | 2509 - T

reference | description | reference | reference
--- | --- | --- | ---
[17] | adaptor | (-).0132 - ALZ | 7002 - TA/9015 - T

reference | description | reference | reference
--- | --- | --- | ---
[18] | valve stem oil seal drift | (-).0132 - W | 4511 - T