C4EB0ZF1 - 206

IDENTIFICATION STRUCTURAL COMPONENTS (3 AND 5 DOOR)

1 - LEFT FRONT BLOCK

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | suspension mounting (front LH) |  | 2+15 | 2.47 | G2 | HLE
2 | wheel arch (front LH) (lengthened part(s)) |  | 1+15 | front 1.17 rear 0.77 | G2 |
3 | chassis leg-tunnel link |  |  | 1.17 | G2 |
4 | centre chassis leg upper stiffener | ** |  | 0.77 | G2 |
5 | chassis leg centre closing panel | ** |  | 1.47 | G2 |
6 | front chassis leg |  | 9+10+12 | 1.47 | G2 |
7 | front block half-panel stiffener |  | 8+13+14+24 | 0.67 | G2 |
8 | front panel bracket |  | 7+13+14+24 | 1.17 | G2 |
9 | chassis leg link |  | 6+10+12 | 1.17 | G2 |
10 | connector(s) support |  | 6+9+12 | 1.47 | G2 | HLE
11 | chassis leg crossmember | ** |  | 0.77 | G2 |
12 | chassis leg link closing panel |  | 6+9+10 | 0.67 | G2 |
13 | front left bumper front bracket | ** | 7+8+14+24 | 1.17 | G2 |
14 | front left bumper rear bracket | ** | 7+8+13+24 | 1.17 | G2 |
15 | wheel arch gusset (front LH) | ** | 1+2 | 0.97 | G2 | HLE
16 | chassis leg/sill link | ** |  | 1.17 | G2 |
17 | engine sub-frame front mounting support |  | 23 | 1.76 | G2 |
18 | chassis leg front partition |  | 23 | 1.17 | G2 |
19 | gearbox support stiffener | ** |  | 2.44 | G2 | HLE
20 | chassis leg rear closing panel | ** |  | 1.47 | G2 | HLE
21 | front wing inner panel | ** |  | 0.97 | G2 |
22 | passenger compartment side front stiffener | ** |  | 0.97 | G2 |
23 | centre chassis leg |  | 17+18 | 2.15 | G2 |
24 | front block half-panel |  | 7+8+13+14 | 0.77 | G2 |
25 | chassis leg double crossmember |  | 11 | 0.97 | G2 | HLE

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) Both faces electro-zinc plated .

(HLE) High strength steel .

2 - RIGHT FRONT BLOCK

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | suspension mounting (front RH) |  | 2+23+14 | 2.47 | G2 | HLE
2 | wheel arch (front RH) (lengthened part(s)) |  | 1+23+14 | front 1.17 rear 0.77 | G2 |
3 | chassis leg-tunnel link |  |  | 1.17 | G2 |
4 | centre chassis leg upper stiffener | ** |  | 0.77 | G2 |
5 | chassis leg centre closing panel | ** |  | 1.47 | G2 |
6 | front chassis leg |  | 9+10+26 | 1.47 | G2 |
7 | front block half-panel stiffener |  | 8+11+12 | 0.67 | G2 |
8 | front panel bracket |  | 7+11+12 | 1.17 | G2 |
9 | chassis leg link |  | 6+10 | 1.17 | G2 |
10 | chassis leg link closing panel |  | 6+9 | 0.67 | G2 |
11 | front block half-panel |  | 7+8+12 | 0.77 | G2 |
12 | bumper bracket (front RH) | ** | 7+8+11 | 1.17 | G2 |
13 | chassis leg/sill link | ** |  | 1.17 | G2 |
14 | wheel arch gusset (front RH) | ** | 1+2+23 | 0.97 | G2 | HLE
15 | engine sub-frame front mounting support |  | 16 | 1.76 | G2 |
16 | centre chassis leg |  | 15+18 | 2.15 | G2 |
17 | chassis leg rear closing panel | ** |  | 1.47 | G2 | HLE
18 | chassis leg front partition |  | 16 | 0.97 | G2 |
19 | engine mounting |  | 20+25 | 2.44 | G2 |
20 | engine mounting side plate |  | 19+25 | 1.95 | G2 |
21 | front wing inner panel | ** |  | 0.97 | G2 |
22 | passenger compartment side front stiffener | ** |  | 0.97 | G2 |
23 | scuttle closing panel (front section) |  | 1+2+14 | 0.77 | G2 |
24 | scuttle closing panel (rear section) | ** |  | 0.67 | G2 |
25 | engine mounting stiffener |  | 19+20 | 1.95 | G2 |
26 | front towing eye |  | 6+9+10 | ø 10 | * |

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

3 - BULKHEAD AND SCUTTLE ASSEMBLY

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | windscreen lower cross member inner panel | ** | 2+4+11 | 0.67 | G2 |
2 | windscreen wiper central support |  | 1+4+11 | 0.97 | G2 |
3 | instrument panel bracket |  | 6+10+12+13 | 0.67 | G2 |
4 | scuttle closing panel (rear section) | ** | 1+2+4+11 | 0.67 | G2 |
5 | fascia crossmember stiffener |  |  | 1.47 | * | HLE
6 | filter bracket deflector |  | 3+10+12+13 | 0.67 | * |
7 | windscreen aperture lower crossmember | ** |  | 0.67 | G2 |
8 | bulkhead crossmember | ** |  | 1.17 | G2 |
9 | accelerator pedal left-hand bracket |  | 14 | 1.76 | * |
10 | bulkhead stiffener |  | 3+6+12+13 | 0.67 | * | HLE
11 | windscreen wiper LH support |  | 1+2+4 | 0.97 | * | HLE
12 | instrument panel bracket |  | 3+6+10+13 | 2.50 | G2 |
13 | upper bulkhead | ** | 3+6+12+13 | 0.67 | * |
14 | lower bulkhead | ** | 9 | 0.77 | G2 |

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

4 - FRONT FLOOR ASSEMBLY

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | RH inner sill |  | 2 | 0.97 | G2 |
2 | right outer front seat cushion rear support | ** | 1 | 1.47 | * |
3 | seat cushion mounting stiffener (front RH) |  | 4 | 1.47 | * |
4 | right front seat crossmember | ** | 3 | 0.77 | * |
5 | right front floor |  |  | 0.57 | G2 |
6 | left front floor |  |  | 0.57 | G2 |
7 | RH rear side rail |  |  | 1.17 | G2 |
8 | tunnel bracket |  | 14+15 | 1.17 | G2 |
9 | chassis leg LH rear |  |  | 1.17 | G2 |
10 | left front seat crossmember | ** | 12 | 0.77 | * |
11 | LH inner sill |  | 13 | 0.97 | G2 |
12 | seat cushion mounting stiffener (front LH) |  | 10 | 1.47 | * |
13 | left outer front seat rear support | ** | 11 | 1.47 | * |
14 | tunnel |  | 15+8 | 1.47 | G2 |
15 | secondary brake mounting stiffener |  | 14+8 | 1.17 | * |
16 | left outer chassis leg | ** |  | 0.97 | G2 |
17 | right outer chassis leg | ** |  | 0.97 | G2 |

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

5 - REAR FLOOR ASSEMBLY

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | passenger compartment side right rear lower closer | ** |  | 1.17 | G2 |
2 | tail lamp housing stiffener (right side) | ** |  | 1.17 | * |
3 | tail panel inner panel |  | 29+30 | 0.97 | G2 |
4 | rear floor stiffener |  |  | 0.97 | * |
5 | front RH side member | ** | 8 | 1.76 | G2 |
6 | rear floor right centre crossmember stiffener | ** |  | 1.95 | G2 | HLE
7 | rear seat right mounting stiffener |  | 9 | 1.47 | * | HLE
8 | right front side member stiffener |  | 5 | 1.76 | G2 | HLE
9 | rear floor |  | 7+21+ 23+24 | 0.57 | G2 |
10 | rear centre seat belt stiffener |  |  | 1.47 | * |
11 | spare wheel pannier right-hand bracket |  |  | 1.17 | G2 |
12 | flanged cross member |  |  | 0.97 | * |
13 | right intermediate side member | ** |  | 0.87 | G2 | HLE
14 | left intermediate side member | ** |  | 0.87 | G2 | HLE
15 | spare wheel pannier left-hand bracket |  |  | 1.17 | G2 |
16 | rear floor centre cross member | ** |  | 0.97 | G2 |
17 | left front side member stiffener |  |  | 1.76 | G2 | HLE
18 | left hand front side member | ** |  | 1.76 | G2 |
19 | crossmember closing panel | ** |  | 0.57 | G2 |
20 | rear floor left centre crossmember stiffener | ** |  | 1.95 | G2 | HLE
21 | rear seat left mounting stiffener |  | 9 | 1.47 | * | HLE
22 | LH rear side member | ** |  | 0.97 | G2 | HLE
23 | bumper lower bracket (rear LH) |  | 9 | 1.17 | G2 |
24 | bumper lower bracket (rear RH) |  | 9 | 0.97 | G2 |
25 | towing eye |  | 26 | ø 10 | * |
26 | RH rear side member |  | 25 | 0.97 | G2 | HLE
27 | passenger compartment bottom rear closer | ** |  | 1.17 | G2 |
28 | tail lamp housing stiffener (left side) | ** |  | 1.17 | * |
29 | rear bumper upper support | ** | 3+30 | 1.17 | G2 |
30 | rear panel |  | 3+29 | 0.87 | G2 |

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

6 - LH OR RH PASSENGER COMPARTMENT SIDE ASSEMBLY - ROOF ASSEMBLY

3 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | roof | ** |  | 0.67 | * |
2 | roof front cross member | ** |  | 0.67 | * |
3 | roof rear cross-member | ** |  | 1.17 | * |
4 | rear pillar stiffener | ** | 11 | 1.47 | * |
5 | windscreen finisher side bracket | ** |  | 0.67 | G2 |
6 | front pillar hinge upper stiffener |  | 7+8+9 | 1.47 | * |
7 | door pillar stiffener | ** | 6+8+9 | 0.97 | * |
8 | front pillar hinge lower stiffener |  | 6+7+9 | 1.47 | * |
9 | front pillar spacer |  | 6+7+8 | 0.97 | * |
10 | water seal bracket | ** |  | 0.67 | G2 |
11 | rear pillar spacer |  | 4 | 1.47 | * |
12 | front inertia reel mounting stiffener |  |  | 1.95 | * | HLE
13 | passenger compartment |  |  | 0.67 | G2 |
14 | rear light outer housing |  | 15 | 0.67 | G2 |
15 | rear light inner housing |  | 14 | 0.87 | G2 |
16 | rear wing upper gutter |  |  | 0.77 | G2 |
17 | rear quarter panel upper stiffener | ** |  | 1.17 | * |

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

5 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | roof | ** |  | 0.67 | * |
2 | roof front cross member | ** |  | 0.67 | * |
3 | roof rear cross-member | ** |  | 1.17 | * |
4 | centre pillar stiffener | ** |  | 1.76 | * |
5 | windscreen finisher side bracket | ** |  | 0.67 | G2 |
6 | front pillar hinge upper stiffener |  | 7+8+9 | 1.47 | * |
7 | door pillar stiffener |  | 6+8+9 | 0.97 | * |
8 | front pillar hinge lower stiffener | ** | 6+7+9 | 1.47 | * |
9 | front pillar spacer |  | 6+7+8 | 0.97 | * |
10 | water seal bracket | ** |  | 0.67 | G2 |
11 | front inertia reel mounting stiffener |  |  | 1.95 | * | HLE
12 | passenger compartment |  |  | 0.67 | G2 |
13 | rear light outer housing |  | 14 | 0.67 | G2 |
14 | rear light inner housing |  | 13 | 0.87 | G2 |
15 | rear wing upper gutter |  |  | 0.77 | G2 |
16 | rear quarter panel upper stiffener | ** |  | 1.17 | * |

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

7 - LH OR RH PASSENGER COMPARTMENT SIDE INNER PANEL ASSEMBLY

3 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | cantrail inner panel | ** |  | 1.17 | * |
2 | windscreen pillar gusset | ** |  | 0.97 | * |
3 | windscreen pillar inner panel | ** |  | 1.17 | * |
4 | rear wing inner panel |  | 10+15+16+ 17+18+19 | 0.67 | * |
5 | door stop yoke closing panel |  |  | 1.76 | * | HLE
6 | sill closer extension | ** |  | 0.67 | G2 |
7 | front jacking point support |  | 8+9 | 2.44 | G2 |
8 | sill web | ** | 7+9 | 0.97 | G2 |
9 | rear jacking point support |  | 7+8 | 2.93 | * |
10 | rear wheel arch stiffener |  | 4+15+16+ 17+18+19 | 0.87 | G2 | HLE
11 | "C" post inner panel | ** |  | 0.67 | G2 |
12 | rear wheel arch rear section | ** | 13+14 | 0.97 | G2 |
13 | rear bumper bracket | ** | 12+14 | 1.47 | G2 |
14 | rear wheel arch |  | 12+13 | 0.67 | G2 |
15 | rear inertia reel mounting stiffener |  | 4+10+16+ 17+18+19 | 1.47 | * | HLE
16 | jacking stiffener |  | 4+10+15+ 17+18+19 | 1.17 | * | HLE
17 | rear back rest striker fixing plate |  | 4+10+15+ 16+18+19 | 1.47 | * |
18 | rear seat belt fastening stiffener |  | 4+10+15+ 16+17+19 | 1.47 | * |
19 | strut support |  | 4+10+15+ 16+17+18 | 2.50 | * | HLE

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

5 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | cantrail inner panel | ** |  | 1.17 | * |
2 | windscreen pillar gusset | ** |  | 0.97 | * |
3 | windscreen pillar inner panel | ** |  | 1.17 | * |
4 | rear wing inner panel |  | 10+15+16+ 17+18+19 | 0.67 | * |
5 | door stop yoke closing panel |  |  | 1.76 | * | HLE
6 | sill closer extension | ** |  | 0.67 | G2 |
7 | front jacking point support |  | 8+9 | 2.44 | G2 |
8 | sill web | ** | 7+9 | 0.97 | G2 |
9 | rear jacking point support |  | 7+8 | 2.93 | * |
10 | rear wheel arch stiffener |  | 4+15+16+ 17+18+19 | 0.87 | G2 |
11 | "C" post inner panel | ** |  | 0.67 | G2 |
12 | rear wheel arch rear section | ** | 13+14 | 0.97 | G2 |
13 | rear bumper bracket | ** | 12+14 | 1.47 | G2 |
14 | rear wheel arch |  | 12+13 | 0.67 | G2 |
15 | rear inertia reel mounting stiffener |  | 4+10+16+ 17+18+19 | 1.47 | * | HLE
16 | jacking stiffener |  | 4+10+15+ 17+18+19 | 1.17 | * | HLE
17 | rear back rest striker fixing plate |  | 4+10+15+ 16+18+19 | 1.47 | * |
18 | rear seat belt fastening stiffener |  | 4+10+15+ 16+17+19 | 1.47 | * |
19 | strut support |  | 4+10+15+ 16+17+18 | 2.50 | * | HLE
20 | centre pillar inner panel | ** |  | 0.67 | * |

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

8 - REMOVABLE PARTS

3 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | tailgate |  | 2 | 0.67 | EZ2 | HLE
2 | tailgate inner panel |  | 1 | 0.57 | G2 |
3 | rear door frame stiffener |  | 4+5+6+7+8 | 1.95 | G2 |
4 | door | ** | 3+5+6+7+8 | 0.67 | G2 | HLE
5 | door inner panel |  | 3+4+6+7+8 | 0.67 | G2 |
6 | door front upper stiffener |  | 3+4+5+7+8 | 0.67 | G2 | HLE
7 | door side impact stiffener |  | 3+4+5+6+8 | 0.57 | * |
8 | door stiffener |  | 3+4+5+6+7 | 1.17 | * | HLE
9 | front wing | ** | 10 | 0.67 | G2 |
10 | front wing front bracket |  | 9 | 1.17 | G2 |
11 | bonnet inner panel |  | 12 | 0.67 | G2 |
12 | bonnet |  | 11 | 0.67 | EZ2 |

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .

5 DOOR SALOON VAN

reference | description | part number for part only | part number for part assembled with | thickness (mm) | coating | type
--- | --- | --- | --- | --- | --- | ---
1 | tailgate |  | 2 | 0.67 | EZ2 | HLE
2 | tailgate inner panel |  | 1 | 0.57 | G2 |
3 | rear door inner panel |  | 7+8 | 0.67 | G2 |
4 | front door inner panel |  | 5+9+10+11 | 0.67 | G2 |
5 | door front upper stiffener |  | 4+9+10+11 | 0.67 | G2 | HLE
6 | bonnet |  | 14 | 0.67 | EZ2 |
7 | rear door stiffener |  | 3+8 | 1.17 | * | HLE
8 | rear door | ** | 3+7 | 0.67 | G2 | HLE
9 | front door | ** | 4+5+10+11 | 0.67 | G2 | HLE
10 | door side impact stiffener |  | 4+5+9+11 | 0.57 | * |
11 | front door stiffener |  | 4+5+9+10 | 1.17 | * | HLE
12 | front wing | ** | 13 | 0.67 | G2 |
13 | front wing front bracket |  | 12 | 1.17 | G2 |
14 | bonnet inner panel |  | 6 | 0.67 | G2 |

ALL MODELS

(**) : Part number for part only .

(*) : Parts not coated .

(G2) : Both faces galvanised .

(EZ2) : Both faces electro-zinc plated .

(HLE) : High strength steel .