C5GG1EF1 - 206 CABRIOLET

REMOVAL - REFITTING FRONT SEAT SLIDES

1 - REMOVAL

REMOVE THE FRONT SEAT .

Remove the fasteners (1) .

Move the slides to gain access to the front fixings .

Remove the front fixings (2) .

Detach the slides assembly (3) to gain access to the seat back control cable .

Unclip the cable (4) at (A) and detach it from the slides assembly .

Remove the slides assembly .

2 - REFITTING

Proceed in the reverse order to removal .

NOTE : the slides must be aligned in order to refit the seat .

REFIT THE SEAT .