C5HG1FK1 - 206

REMOVAL - REFITTING BLOWER SPEED RESISTOR UNIT

1 - REMOVAL

Disconnect the battery .

Remove the glove box .

Move the air intake control to the RECIRCULATION position .

Insert your hand into the air intake duct .

Take hold of the blower speed resistor unit (1) by the protective lid and release it from the duct by turning towards the left .

Pull towards you to detach it from the duct accompanied by the harness .

Press on either side of the connector to release it, pull the connector .

Disconnect the resistor .

2 - REFITTING

Proceed in the reverse order to removal .