B1HG1HK1 - 206 DW8 ENGINE DW10TD ENGINE TU ENGINE

REMOVAL - REFITTING FUEL TANK

1 - REMOVAL

Empty the tank using draining equipment .

Place the vehicle on a lift with rear wheels suspended .

Remove :

- the right hand rear wheel
- the mud shield

Remove : The securing bolts (1) (Fuel filler neck) .

Remove the intermediate silencer .

Remove the metal heat shield (2) .

Unclip the hand brake cables from the tank .

Remove the tank securing bolts (3) .

Lower the tank without removing it .

Disconnect :

- the pipes connected to the tank and to the filler neck
- the fuel gauge connector

Remove : Tank and filler neck assembly .

2 - REFITTING

Re-assemble in the reverse order to dismantling .