E2AK0VK1 - 206

LIFTING

1 - SPECIAL TOOLS

[1] cross beam (-).0010 .

2 - POSITIONING CHASSIS STANDS

2 - 1 - AT THE FRONT

Take the load on the sill with the crossmember as close as possible to the locating plate .

Position the axle stand in the location provided for lifting the vehicle using the jack .

NOTE : to have 2 wheels suspended, repeat the operation on the other side .

2 - 2 - AT THE REAR

Take the load on the sill with the crossmember as close as possible to the locating plate .

Position the axle stand in the location provided for lifting the vehicle using the jack .

NOTE : to have 2 wheels suspended, repeat the operation on the other side .

3 - RAISING FROM ONE SIDE

Position the axle stand in the location provided for lifting the vehicle using the jack .

NOTE : to have 4 wheels suspended, repeat the operation on the other side .

4 - LIFTING ON A 2 POST LIFT

Place the lift pads on each locating plate .

5 - SINGLE OR TWO POST LIFT

WARNING : removal of units (power unit, rear suspension ...) can cause movement of the centre of gravity: use a single or two post lift fitted with clamps to hold the body to the lift arms .

Position the clamps under the lifting plates with the tightening bolt heads towards the outside of the vehicle .

Place the clamps in the cut-out provided for the jack .

Tighten the clamps using the pin and after tightening insert the pin into the hole (A) .