C4AG0CF1 - 206

REMOVAL - REFITTING GRILLE

1 - REMOVAL

Open the bonnet .

Remove :

- the fasteners (1)
- the grille (upper part) (2)
- the bolt connecting to the cassette and fan assembly (3)
- the fasteners (4)

Unfasten the grille (5) (In the following order) :

- at the centreline of the vehicle
- at the end of each headlight

Remove the grille (5) .

2 - REFITTING

Insert and clip the two ends in the left and right housings of the front wing supports .

Clip the grille :

- at the bottom of the end of the headlight : tighten the bolts (4)
- at the centreline of the vehicle under the badge

Tighten the bolt (3) which secures the upper rigid plate connecting with the fan assembly cassette .