B2CG6VK1 - 206 MA GEARBOX

REMOVAL - REFITTING GEARBOX CONTROLS

1 - SPECIAL TOOLS

[1] Tool for unclipping 10 dia. ball joints (-).0216 G1 .

[2] Tool for unclipping 13 dia. ball joints (-).0217 G2 .

[3] Clip pliers (CLIC (-).0172) .

2 - REMOVAL

Unclip the gaiter (1) from the central console .

Remove the knob-gaiter assembly by pulling upwards (A) .

Remove the bolts (2) .

TU1JP ENGINE EMISSION CONTROL CEE 95 TU3JP ENGINE EMISSION CONTROL CEE 95

Remove :

- the collar (3) (using the tool [3])
- the oil vapour breather pipes (at (B))
- the air cleaner assembly (4)

TU5JP ENGINE EMISSION CONTROL CEE 95

Remove :

- the collars (3) (using the pliers [3])
- the oil vapour breather pipes (at (B))
- the air cleaner (4)
- the air outlet union

ALL MODELS

Remove :

- the rods (5) (using the tool [1])
- the push rod (6) (using the tool [2])

Remove the bolt (7) .

Raise the vehicle .

Remove : The exhaust clamp (8) .

Remove :

- the exhaust clamp (9)
- the bolts (10)
- the nuts (11)
- the gear lever

3 - REFITTING

Use ESSO NORVA 275 grease to coat the hinges (12) .

Use ESSO 3106 grease to coat the hinge (13) .

Tighten the nut (14) to 0.8 da.Nm .

Continue the fitting operations in the reverse order to removal .

Use LOCTITE FRENETANCH to coat the thread of bolt (7) .

Tighten the bolts (2) to 0.8 daN.m .

Refit the knob-gaiter assembly .