C4CH2EF1 - 206 CABRIOLET

REPLACEMENT INNER SILL INNER SIDE MEMBER STIFFENER EXTENSION

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZE WELDING TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- OUTER SILL
- outer side member insert

2 - IDENTIFICATION OF REPLACEMENT PARTS

(1) Inner sill .

(2) Inner side member stiffener extension .

(3) Front seat slide fastening support .

3 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

(1) Inner sill .

(2) Inner side member stiffener extension .

(3) Front seat slide fastening support .

4 - PREPARATION OF THE NEW PART

5 - CUTTING OUT

6 - RELEASING

7 - ADJUSTMENT

8 - WELDING