B2CH0JK1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING DRIVE SHAFT SEALS

1 - REMOVAL

DRAIN THE GEARBOX .

REMOVE THE DRIVE SHAFTS .

Extract the right hand transmission seal ; USING THE TOOL [5] .

Remove the left hand transmission seal by pushing it towards the inside of the housing, using a pin punch and a hammer .

2 - REFITTING

Lubricate a new lip seal .

Refit the right hand transmission seal ; USING THE TOOL [9] - [10] .

Lubricate a new lip seal .

Refit the left hand transmission seal ; USING THE TOOL [7] - [8] .

REFIT THE DRIVE SHAFTS .

FILL GEARBOX WITH OIL AND ENSURE CORRECT LEVEL .

Initialise the oil wear counter (Follow the 2000 diagnostic equipment procedure) .