E3AK06K1 - 206

MAINTENANCE CONDITIONS

1 - WARRANTY INSPECTION (FIRST SERVICE)

| normal servicing - arduous conditions maintenance
--- | ---
petrol engine(s) / diesel engine(s) | 10000 km, 6000 miles, or 6 months

2 - SERVICING

| normal servicing | arduous conditions maintenance
--- | --- | ---
petrol engine(s) | every 30000 km, every 20000 miles, or every 2 year(s) | every 20000 km, every 12000 miles or every year(s)
diesel engine(s) (direct injection) | every 20000 km, every 12000 miles, or every 2 year(s) | every 15000 km, every 10000 miles or every year(s)
diesel engine(s) (except direct injection) | every 15000 km, every 10000 miles or every 2 year(s) | every 10000 km, every 6000 miles, or every year(s)

3 - INTERMEDIATE VISIT

Taking into account the interval between services, an intermediate visit for topping up the engine oil and carrying out visual checks should be carried out mid-way between two services .