B3BG0PK1 - 206

REMOVAL - REFITTING FRONT ANTI-ROLL BAR MOUNTING

1 - REMOVAL

TU ENGINE

Remove :

- the exhaust ball joint bolts

Remove :

- the nuts (1)
- the bolts (2)
- the anti-roll bar

2 - REFITTING

2 - 1 - ANTI-ROLL BAR BEARINGS

The anti-roll bar is supported in two flexible bearings (4) .

Lateral and horizontal positioning is guaranteed by means of two flats (A) on the inside of the mounting and by mouldings (B) on the bar section .

A clamp (3) retains the assembly .

Open the bearing .

Align the internal flats (A) with the mouldings (B) on the anti-roll bar (one on either side) .

2 - 2 - ANTI-ROLL BAR

Proceed in the reverse order to removal .

Tightening torque(s) :

- mounting (1) link to anti-roll bar : 3.6 da.Nm
- anti-roll bar bearing(s) mounting (2) : 10.4 da.Nm