C4CH1GF1 - 206

REPLACEMENT OUTSIDE TEMPERATURE SENSOR

1 - REMOVAL

Remove :

- the mirror (right)
- the mirror glass

Remove the bolts (1) .

Remove the bolts (2) .

Move aside the assembly at (A) using a plastic spatula .

Detach the sensor (3) and the harness to obtain a sufficient length of wire .

Cut the black wires of the sensor at (B) and restore the electrical connection using soldering connectors .

Insulate the connector with the heat shrink sleeve .

2 - REFITTING

Proceed in the reverse order to removal .

Test all the electrical functions several times .