C7AP0PV1 - 206

FITTING CAR PHONE GSM

1 - PRESENTATION

(1) Aerial GSM .

(2) Central unit 8 W (According to specification) .

(3) Speaker .

(4) Central unit 2 W (According to specification) .

(5) Phone bracket .

(6) Phone console .

(7) Microphone .

1 - 1 - CAR PHONE 8 W, PART NO. 9707.X1

description | reference
--- | ---
aerial GSM | 1
central unit 8 W | 2
speaker | 3
handset rest | 5
microphone | 7
connection unit and wiring | 8
handset extension lead | 9
instrument panel | 10
battery +ve (red) | 11
ignition controlled +ve (green) | 12
earth (black) | 13
audio MUTE (yellow/black) | 14

1 - 2 - CAR PHONE 2 W

description | reference
--- | ---
aerial GSM | 1
speaker | 3
central unit 2 W | 4
handset rest | 5
microphone | 7
mobile telephone connection cable | 9a
mobile phone | 10a
battery +ve | 11
ignition controlled +ve | 12
earth | 13
audio MUTE | 14

2 - FITTING : AERIAL (1)

2 - 1 - ROOF AERIAL

Partly remove the upper section of the tailgate aperture seal (15) .

Special feature - 5-door :

- partly remove the upper section of the right and left rear door seals (16)

Remove :

- the right quarter panel trim (17)
- the right side trim (18)

NOTE : the headlining must be handled carefully to prevent any damage .

Lower the headlining (19) without folding it and keep it in this position using 2 shims (20) .

Mark and drill the roof, in the centreline, to a diameter of 14 mm observing the dimension (a) of 60 mm in relation to the edge of the roof .

Protect the hole using anti-corrosion product .

WARNING : strip back the roof panel on the interior around the hole .

Protect the bared metal using a PA C15 type electro-conductive compound (Part No. 9734.08) .

Secure the aerial taking care not to deform the roof and directing the wire to the right .

Route the aerial wire under the headlining to the right rear wheel arch front trim (21) .

Special feature - Assembly 2 W (22) :

- route the aerial cable in the right interior side member, along the original harness, to the glove compartment

2 - 2 - BUMPER AERIAL

For vehicles fitted with the electric sliding sun roof or the panoramic roof .

Open the tailgate .

Remove :

- the fasteners (23)
- the rear mud shields
- the fasteners (24)
- the electrical connection (25)

Remove the rear bumper .

Bond the aerial sensors (26) inside the bumper using the following product :

- cartridge of adhesive : Part No. 9724.51
- application gun : Part No. 9724.52

The sensors must be in contact with the sides of the bumper .

Secure the wire on the bumper using the adhesive clips supplied and form a loop with the surplus wire between the aerial sensors .

Remove the luggage compartment trim (right side) .

Remove the air extractor (27) (right side) .

Drill a 14 mm diameter hole at the bottom .

Fit the air extractor .

Fit the bumper .

Check the operation of the lights .

Route the aerial wire (28) in the extractor to the right rear wheel arch front trim (29) .

Insert the grommet supplied onto the aerial wire and push it to position it in the hole (use soap to make fitting easier) .

Check that the grommet is fitted correctly to obtain perfect sealing .

Special feature-Fitting : 2W (30) .

Use an extension lead in addition to the bumper aerial :

- Part No. 9707.K8 (length 2 m)
- Part No. 9707.S9 (length 3 m)

Route the aerial wire in the right interior side member, along the original harness, to the glove compartment .

3 - FITTING : CAR PHONE

3 - 1 - CAR PHONE 8 W (2) - (5) (PART NO. 9707.X1)

Disconnect the battery .

Mark and drill the centre rib (31) of the right rear wing inner panel observing the dimension (b) of 60 mm to secure the central unit .

WARNING : protect the exposed metal with an anti-corrosion product .

Connect the connection unit (8) to the central unit (2) .

Connect the earth wire (black) (13) using a, 8 mm diameter, round terminal to the earth grommet (32) with a bolt part number 6924.88 .

Refit the boot side trim and mark the holes made earlier .

Secure the central unit (2) .

Route the permanent positive wire (red) (11) under the boot side trim to the rear of the vehicle .

Inside the wheel arch (Rear RH) :

- cut the ends of the bolts
- check that there is no contact between the bolts and any mechanical component
- apply an underseal product to each bolt

Remove the luggage compartment side trim (On the left-hand side) .

Route the permanent positive wire (red) (11) under the original filler neck (33) to the boot light 2-way brown connector (34) .

Connect the (red) wire (11) to wire no. BH15 at terminal 1 of the boot light using a Raychem sleeve .

Partly remove the door aperture seals (right side) .

Partly unclip the carpet .

In the right interior side member, along the original harnesses, route the following wires :

- ignition controlled +ve (green) (12) (to the passenger compartment fuse box)
- audio MUTE (yellow/black) (14) (to the radio)
- handset extension lead (9) (to the fascia centre console)

Remove the access flap (35) .

Remove the bolts (36) from the passenger compartment fuse box (37) .

Remove the passenger compartment fuse box (37) .

Unclip the passenger compartment fuse box double lock (38) (37) .

Connect the ignition controlled positive wire (green) (12), using a terminal Part No. 6542.FR to terminal B5 of the passenger compartment fuse box .

Clip the double lock (38) .

Insert the 10 A fuse at terminal 5 .

3 - 2 - CAR PHONE 2 W (4) - (5)

Disconnect the battery .

Secure the central unit (4) of the hands-free kit to the left-hand side of the glove compartment (Next to the light ; According to specification) .

Connect the mobile phone connection cable (9a) to the central unit (4) .

Route the wire(s) :

- earth (13) (to the door hinge pillar)
- ignition controlled +ve (12) (to the passenger compartment fuse box)
- battery +ve (11) (to the passenger compartment fuse box)
- audio MUTE (14) (to the radio)
- mobile telephone connection cable (9a) (to the fascia centre console)

Partly remove the bottom section of the front door aperture seal (39) .

Partly unclip the carpet (40) .

Connect the earth wire (13) using a 8 mm diameter round terminal to the earth grommet (41) MC22 .

Remove the access flap (35) .

Remove the bolts (36) from the passenger compartment fuse box (37) .

Remove the passenger compartment fuse box (37) .

Unclip the double lock (38) on the passenger compartment fuse box (37) which corresponds to fuses 5 and 10 .

Connect :

- the ignition controlled positive supply (12) using a terminal part number 6542.FR to terminal B5
- the permanent positive supply (11) using a terminal part number 6542.FR to the terminal A10

Clip the double locks (38) .

Insert a 5 A fuse at terminal 5 and a 10 A fuse at terminal 10 .

4 - FITTING : MICROPHONE (7)

Remove the left windscreen pillar trim .

Route the microphone wire (7) :

- along the left windscreen pillar
- under the fascia to the right door hinge pillar

Special feature - Car phone 2 W :

- connect the microphone wire to the central unit of the hands-free kit secured to the glove compartment

Special feature - Car phone 8 W :

- route the microphone wire in the right interior side member along the original harness to the central unit secured on the right rear wing inner panel
- connect the microphone wire to the 8 W central unit

5 - FITTING : SPEAKER (3)

Secure the speaker (3) under the glove compartment from the inside .

Special feature - Car phone 2 W :

- connect the speaker wire (3) to the central unit of the hands-free kit secured to the glove compartment

Special feature - Car phone 8 W :

- route the speaker wire (3) in the right interior side member along the original harness to the central unit secured on the right rear wing inner panel
- connect the speaker wire (3) to the 8 W central unit

6 - MUTE CONNECTION (14) (ACCORDING TO SPECIFICATION)

Remove the radio .

Connect the audio mute wire (14) using a terminal part no. 6542.T9 to terminal no. 1 of the radio 8-way black connector (42) .

7 - FITTING : CAR PHONE CONSOLE (6)

Remove :

- the radio aperture cover/the radio (43) (according to specification)
- the upper central panel (44)
- the 2 bolts (45)
- the centre panel (46)

Route the phone connection wire (9)-(9a) in the tapping (47) of the console (6) and keep it in place using adhesive tape .

Secure the front section of the console (6) using the 2 bolts (48) of the air conditioning control unit (49) .

Using a small file, make two small notches on the lower edge (50) of the centre panel (46) opposite the telephone console securing lugs (6) .

Insert the clip (51) between the fascia (52) and the console slot (6) to keep the rear section in place .

7 - 1 - SPECIAL FEATURE - CAR PHONE 8 W

Position the handset rest (5) in the upper section of the console (6) .

Mark the securing holes .

Drill pre-holes (metal bracket incorporated in the console) .

Secure the handset rest .

Secure the handset extension lead unit on the console .

Fit the handset (10) on its rest (5) .

Connect the handset to the extension lead unit .

7 - 2 - SPECIAL FEATURE - CAR PHONE 2 W

Position the handset rest (5) in the centre section of the console (6) .

Mark the securing holes .

Drill pre-holes (metal bracket incorporated in the console) .

Secure the handset rest .

Fit the mobile telephone (10a) on its rest (5) .