B3CG0SK1 - 206

REMOVAL - REFITTING FRONT LOWER ARM

1 - SPECIAL TOOLS

[1] Set of 2 spring retaining rods (-).0918Z .

[2] Swivel ball joint uncoupling lever (-).0622 .

2 - REMOVAL

Position : The spring retaining rods .

Lift and support the vehicle with front wheels suspended .

Remove :

- the wheel
- fastening (1) of the ball joint to the pivot

Extract the wishbone ball joint from the pivot using the tool [2], taking care not to damage the ball joint boot with the chain of the tool [2] .

Lock the lower wishbone in the lower position (Use a socket) .

{{N11661}} maintenir le pivot vers l'arrière avec un fil de fer, afin de ne pas endommager la rotule de pivot .

Remove :

- arm front articulation fastener (2)
- the fastener (3)
- {{n11662}} le bras inferieur

3 - REFITTING

Position the lower arm fitted with its flexible bushes and including that for the ball joint .

Refit the bolts which secure the wishbone to the sub-frame .

Tighten :

- front fastener to 14 daN.m
- rear fastener to 14 daN.m

Ensure that the boot protecting the ball joint is in good condition (no cuts on the boot and securing clip present) .

Clean the ball joint taper, move the boot from the top to the bottom so that it regains its flexibility, position the boot in the fully extended position .

Engage the lower arm ball joint in the pivot, without forgetting the ball joint protector which must be positioned correctly (indexer) .

Fit the ball joint bolt and a new nut : Tightening torque to 4 da.Nm .

Tighten the wheel bolts to 8.5 da.Nm .

Return the vehicle to its wheels .

Remove : The spring retaining rods .