B--G0JK1 - 206 EW10J4 ENGINE

REMOVAL - REFITTING ANCILLARY DRIVE BELT

1 - SPECIAL TOOLS

[1] setting rod for dynamic roller (-).0189-E .

2 - REMOVAL

EW10J4 ENGINE

Slacken the belt by turning the bolt (1) .

Pin the dynamic tensioner (2) using the tool [1] .

Remove the belt (if present) .

IMPERATIVE : check that the rollers (3) and (4) turn freely (no play and no tight spots) .

3 - REFITTING

Fit the belt .

Take care that the belt is correctly located in the grooves of the various pulleys .

Remove the rod [1] by pulling gently on the belt span .