C5JG0DF1 - 206 CABRIOLET

REMOVAL - REFITTING OF THE FRONT SEAT BELT

1 - REMOVAL

Disconnect the battery .

Remove :

- THE REAR SEAT
- THE REAR SEAT BACK REST
- THE REAR QUARTER PANEL SIDE TOP TRIM
- THE REAR QUARTER PANEL SIDE TRIM PANEL

Disconnect the pretensioner (1) .

Remove the fasteners (2) - (3) .

Remove the seat belt .

2 - REFITTING

Proceed in the reverse order to removal .

Tighten the fasteners (2) - (3) to 3 ± 1 da.Nm .