B2CG77K1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING GEARBOX OUTPUT SPEED SENSOR

1 - REMOVAL

NOTE : do not drain the gearbox .

Disconnect the battery + terminal .

WARNING : the connector mounting (3) is fragile .

Remove :

- the front left-hand wheel
- the bolt (1)
- automatic gearbox output speed sensor (2)
- the connector (3)

2 - REFITTING

Replace the sensor o ring (2) .

Fit :

- the connector (3)
- automatic gearbox output speed sensor (2)
- the bolt (1) (tightening torque 1 da.Nm)
- the front left-hand wheel

Reconnect the positive terminal of the battery .