B1EB04K1 - 206 TU5JP ENGINE TU1JP ENGINE TU3JP ENGINE

DATA - IDENTIFICATION CAMSHAFTS

The camshafts possess two types of identification :

- marking on the end of the shaft (A), flywheel end
- colour identification (B), (C), (D)

Colour identification (B) :

- this marking is located on the cam ring, flywheel end

Colour identification (C) - (D) :

- this marking is located on the flat section, between bearing no. 2 and the inlet cam A1

engine type | colour identification (B) | colour identification (C) | colour identification (D) | marking on the end of the shaft (A)
--- | --- | --- | --- | ---
TU9 | - | yellow | - | E
TU9M | - | - | yellow | 4
TU1 - TU3 | - | green | - | 1
TU1M | - | blue | - | M
TU1M+ to 2616141 TU3JP to 2333357 | orange | - | - | Y
TU1JP | white | - | - | 7
TU2.4 | - | white | - | 2
TU2J2 | - | - | black | J
TU3A | - | orange | - | A
TU3S | - | black | - | R
TU3.2 TU3F2 | - | brown | - | B
TU3M TU3FM | - | pink | - | 3
TU3MC TU3FMC | - | - | pink | C
TU3J2 | - | beige | - | Z
TU3JP from 2333358 TU1M+ from 26161142 | - | - | beige | H
TU5JP injection control unit MP5.1 | green | - | - | 5
TU5JP injection control unit MP5.2 to 344273 | blue | - | - | 6
TU5JP/L3 from 344274 | - | - | brown | T
TU5J2 | - | - | black | J

camshaft seal bearings
distance (mm) | nominal | repair 1
--- | --- | ---
ø F -0.025-0.050 | ø 36 | ø 35.8

Grinding of camshaft seal bearings to 0.2 mm (production seals fitted) .