B1FG03K1 - 206 TU3JP ENGINE TU1JP ENGINE TU5JP ENGINE TU5JP4 ENGINE

REMOVAL - REFITTING OIL FILTER

1 - REMOVAL

WARNING : as draining is carried out when warm, beware of nearby heat sources .

Cover (1) .

Tabs (2) .

Cover gasket (3) .

Filter cartridge (4) .

WARNING : be careful to avoid splashes of oil onto the catalytic converter .

Slacken the cover (1) .

NOTE : the tabs (2) are designed to hold the cover on a 27 mm pin so that the cover can be removed without burning your hands on the catalytic converter .

Detach the cover and remove it .

Detach the filter from the cover, pull it in the direction of the arrows (A) .

Remove the seal (3) .

WARNING : take care not to damage the seal groove .

2 - REFITTING

Fit :

- a new seal (3)
- a new filter element
- the cover fitted with its filter element ; tightening torque 2.8 da.Nm