C4BH2ZF1 - 206 CABRIOLET

REPLACEMENT REAR WING

IMPERATIVE : this vehicle has been designed using the mig brazing process technique ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Removal - refitting :

- REAR BUMPER
- tail lamp
- QUARTER LIGHT - REAR QUARTER PANEL WINDOW MECHANISM
- DOOR STRIKER
- door aperture seal
- TAILGATE SEAL
- REAR QUARTER PANEL INTERIOR WEATHERSTRIP SEAL
- REAR QUARTER PANEL EXTERIOR WEATHERSTRIP
- FUEL TANK (right-hand side)
- REAR QUARTER PANEL WEATHERSTRIP END PIECE
- rear mud shield
- wing protector side moulding
- front seat belt inertia reel

Remove-refit trim :

- rear wing inner panel

Detach the electrical harnesses .

Protect :

- the fuel pipes (right side)
- the front carpet and boot carpet

2 - IDENTIFICATION OF REPLACEMENT PARTS

Rear wing .

3 - COMPOSITION REPLACEMENT PARTS

(1) : Rear wing .

(2) : Rear wing stiffener .

4 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Rear wing .

5 - PREPARATION OF THE NEW PART

6 - CUTTING OUT

7 - RELEASING

8 - ADJUSTMENT

9 - WELDING

10 - SEALING

11 - PROTECTION