B3EB0MK1 - 206

RECOMMENDATIONS POWER STEERING FLUID (SERVICE)

The hydraulic fluid DEXRON 2 can be used for the following vehicles (Temperate climates) :

- 106 - 206 - 306
- 406 - 607 - 806
- PARTNER - EXPERT - BOXER

NOTE : for versions for very cold climates: the hydraulic fluid TOTAL FLUIDE LDS H50126 or the hydraulic fluid PENTOSIN CHF11S must be used .

For the following vehicles :

- 307 all models
- 406 - 607 versions for very cold climates

IMPERATIVE : use only the hydraulic fluid TOTAL FLUIDE LDS H50126 instead of the hydraulic fluid PENTOSIN CHF11S .

WARNING : the hydraulic fluids TOTAL FLUIDE LDS H50126 or PENTOSIN CHF11S can be mixed together ; the hydraulic fluid DEXRON 2 cannot be mixed with any of the hydraulic fluids mentioned above .