B1CB1VK1 - 206 TU5JP ENGINE TU1JP ENGINE TU3JP ENGINE

DATA IDENTIFICATION CONNECTING RODS

1 - ENGINES - 1ST GENERATION

engines - 1st generation
engine type | TU9 | TU1 - TU2.4 | TU2J2 | TU3 | TU5
--- | --- | --- | --- | --- | ---
distance (mm) | nominal
ø A + 0,016 + 0 | 41,128 | 48,655
ø B + 0,017 + 0 | 17,939 | 19,463
C ± 0,07 | 122,8 | 112,3 | 133,5 | 126,8 | 133,5

NOTE : the connecting rods of the 1st generation TU5 engines are carried over to the 2nd generation .

2 - ENGINES - 2ND GENERATION

engines - 2nd generation
engine type | TU1 | TU3
--- | --- | ---
distance (mm) | nominal
ø A + 0,016 + 0 | 48,655
ø B + 0,011 + 0 | 19,463
C ± 0,05 | 125,3 | 140,25

The new connecting rod is fitted with an oil jet (1) for spraying the underneath of the piston .

The connecting rod is fitted with a new drilled half shell .