C5JH0AF1 - 206

MODIFICATION TO THE REAR WHEEL FRONT MUD GUARD

1 - REMOVAL OF THE LOWER SECTION OF THE FRONT MUD GUARD

NOTE : when repairing a vehicle in service, this operation avoids replacement of the part on both sides of the vehicle .

1 - 1 - OPERATION

Remove the rear mud guard concerned .

Cut the vertical section (A) of the front mud guard under the corner of the securing flap on the passenger compartment side (B) following the cutting line (C) .

Refit the rear mud guard .