C4CH1UF1 - 206 CABRIOLET

REPLACEMENT DOOR OPENING FINISHER

1 - REMOVAL

Dislodge the door opening seal (1) .

Gradually detach the door opening finisher (2) (taking care not to damage the paint) using a spatula (A) .

2 - REFITTING

Clean the bearing surface in order to remove traces of dirt .

Heat to a moderate temperature the new finisher (radiant panel or hot air gun) .

By means of a pinching action and using a carpenter's rule, measure the starting dimension for positioning the finisher (dimension (3)) .

Identification of the position with adhesive tape .

Peel off the adhesive protection paper on the finisher .

Position the finisher (2), starting with the identification with the adhesive tape (4), then following the depression (5) of the external side member .

Press the whole of the contact surface, using force .

Remove the adhesive tape used for identification .

Place the door opening seal back in position .