B2GT00K1 - 206 DAM FROM : 860688

MODIFICATION WHEEL BOLTS

1 - PARTS AFFECTED BY THE CHANGE

Light-alloy wheels .

Spare wheel .

Wheel bolts .

2 - IDENTIFICATION

(1) Wheel bolt, type a mixed fitting .

This new wheel bolt type a mixed fitting is used to tighten wheels of the following types :

- light-alloy wheels (with flat span mounting)
- steel spare wheel (with conical span mounting)

2 - 1 - EARLIER ASSEMBLY

(2) Standard wheel bolts .

(2) Standard wheel bolts .

(3) Steel spare wheel .

(4) Light-alloy wheels .

2 - 2 - LATER ASSEMBLY

(1) Mixed fitting wheel bolts .

(3) Steel spare wheel .

(4) Light-alloy wheels .

This modification involves the following modifications :

- addition of a spot facing in light alloy wheel fixture recess
- elimination of inserts allowing spare wheel to be fitted with flat span bolts

3 - INTERCHANGEABILITY

The new light alloy wheel accepts both the old and the new bolt .

WARNING : the old light alloy wheel is not compatible with the new bolt .

Parts Division supplies both assemblies .