B1DB2LK1 - 206 TU5JP ENGINE TU1JP ENGINE TU3JP ENGINE

DATA ROCKERS

1 - ROLLER ROCKERS

The rocker fingers have been replaced by rocker arms fitted with a bearing for making contact with the cams; they are known as ROLLER ROCKER ARMS .

WARNING : avoid direct contact between hands and rocker bearing tracks .

2 - ADJUSTING SCREW

(1) Rockers .

(2) Bolt(s) M9 .

(3) Bolt(s) M6 .

The adjusting bolts have been modified: the M6 (3) bolts are gradually replaced with bolts .

IMPERATIVE : DEVELOPMENT OF THE TIGHTENING TORQUES .