C5KG0JF1 - 206

REMOVAL - REFITTING ELECTRIC SUN ROOF MOTOR

1 - REMOVAL

Open the sun roof panel trim .

Remove :

- the sun visors
- the sun visor retaining hooks
- the roof console
- partly : remove the screen pillar trim
- the front grab handles
- the sun roof frame finishing seal

Release the headlining from the front door seals .

WARNING : lower the headlining at the front taking care not to fold it .

Disconnect the electrical connection (1) .

Remove the fasteners (2) .

Uncouple the motor from the mechanism .

Release the motor from the left .

2 - REFITTING

IMPERATIVE : check : the coupling of the motor to its mechanism .

Proceed in the reverse order to removal .