C4CH2FF1 - 206 5 ESTATE

IDENTIFICATION PASSENGER COMPARTMENT

reference | description | Part No. | thickness (mm) | comment(s)
--- | --- | --- | --- | ---
| left passenger compartment side assembly | yes |  | 1 to 13
1 | left passenger compartment side | no | 0,67 |
2 | left splash seal front support | yes | 0,67 |
3 | left windscreen trim side support | no | 0,67 |
4 | left light housing closer | no | 0,76 |
5 | left b-post stiffener | yes | 1,76 | 5+6
6 | left b-post upper stiffener | no | 1,76 |
7 | rear left light inner housing | yes | 0,97 | 7+8
8 | boot left strut support | no | 1,76 |
9 | rear left bumper support | yes | 1,17 |
10 | side member closer left extension | yes | 0,67 |
11 | front wing support angle bracket | yes | 1,5 |
12 | rear left wing lower drip moulding | yes | 0,77 |
13 | rear left door striker fixed stiffener | no | 1,17 | +1
14 | passenger compartment side front stiffener | yes | 0,97 |