C5EG0TF1 - 206 CABRIOLET

REMOVAL - REFITTING NUMBER PLATE LIGHT

1 - REMOVAL

Open the luggage compartment .

REMOVE THE BOOT COVER TRIM .

Close the boot .

Switch on the ignition .

IMPERATIVE : leave the ignition on throughout the operation .

NOTE : do not forget to unlock the roof strikers and to unroll the screen (luggage cover) .

Press the roof control button until the boot cover opens, then release it .

Place your hand between the upper cover and the lower cover of the boot .

Press the translucent housing (1) then tilt it to detach it from the support .

Disconnect the connector (2) .

Close the boot cover by pressing the roof control button .

Open the luggage compartment .

Using a thin blade [1], push on the lugs (3) to release the support (4) by lifting it .

Detach and remove the support (4) .

2 - REFITTING

Fit the translucent housing on the support .

Engage then clip the support on the lower panel .

Re-connect the connector (2) .

Close the boot .

Check that the number plate lamps operate .

Lock the roof strikers .