C5EG0UF1 - 206 CABRIOLET

REMOVAL - REFITTING BOTTLE STORAGE COVER

1 - REMOVAL

Tilt the bottle storage cover (1) to the open position .

Hold the bottle storage cover at the top (A) .

Moderately tap the bottle storage cover at the bottom (B) .

Remove the bottle storage cover (1) .

2 - REFITTING

Refit the bottle storage cover (1) .

Place your hand inside the opening .

Push on the pin (2) in the notches (3) .

Take care to engage the pin on the notches correctly, checking by means of a closing movement .