E4AT00K1 - 206

NEW COOLANT

Adoption of a new long life REVKOGEL 2000 or GLYSANTIN G33 coolant :

- from build code 8576XX : all models (not 106 ELECTRIC - PARTNER ELECTRIC - BOXER)
- from build code 8566XX : for 106 ELECTRIC - PARTNER ELECTRIC

The products do not require periodic draining/refilling .

These new products are diluted 50 % with demineralized water for all countries and provide protection up to -35 ° c .

NOTE : the old products are still sold for vehicles prior to adoption of the new product, consequently the replacement frequency remains unchanged (see maintenance booklet) .