B1BG2AK1 - 206 D4D ENGINE MERCOSUR

IDENTIFICATION TENSION OF THE BELTS

1 - SPECIAL TOOLS

[1] (-).0192 tension measuring equipment .

2 - IDENTIFICATION

NOTE : all the belts are polyvee type .

(A) Crankshaft .

(B) Alternator .

(T) Tension checking points .

POWER STEERING

(A) Crankshaft .

(B) Alternator .

(C) Power steering pump .

(H) Roller tensioner .

(T) Tension checking points .

AIR CONDITIONING

(A) Crankshaft .

(B) Alternator .

(D) Air conditioning compressor .

(H) Roller tensioner .

(T) Tension checking points .

POWER STEERING AIR CONDITIONING

(A) Crankshaft .

(B) Alternator .

(C) Power steering pump .

(D) Air conditioning compressor .

(G) Roller tensioner .

(H) Roller tensioner .

(T) Tension checking points .

ALL MODELS

3 - TENSION OF THE BELTS

engine type | D4D | D4D | D4D | D4D
--- | --- | --- | --- | ---
special features | without | power steering | with air conditioning | power steering + with air conditioning
new belt (units Hertz) | 260 ± 5 | 210 ± 5 | 210 ± 5 | 210 ± 5
re-used belt (units Hertz) | 260 ± 5 | 210 ± 5 | 210 ± 5 | 210 ± 5