E5AB1EK1 - 206 DW10TD ENGINE

PRESENTATION TOOLING CLUTCH

1 - SPECIAL TOOLS

clutch kit
reference | description | reference | reference
--- | --- | --- | ---
[1] | kit | (-).0216 - ZW | 9040 - T
[1a] | gearbox pins/guide | (-).0216 - A | (-).0216 - A
[1b] | stop removal pliers | (-).0216 - B | (-).0216 - B
[1c] | - engine and gearbox mandrel - cone for stop | (-).0216 - C | (-).0216 - C
[1d] | - stop unclipping/clipping drift - stop clip repositioning retainer | (-).0216 - D | (-).0216 - D
[1e] | hydraulic control clutch stop clipping tool 605 (version TC) and 406 | (-).0216 - E | (-).0216 - E
[1f] | - gearbox hydraulic control protector cone ME5T (long) - gearbox hydraulic control protector cone MG5T (short) and ML5T | (-).0216 - F | (-).0216 - F
[1g] | cable control ball joints unclipping tool(s) | (-).0216 - G | (-).0216 - G
[1h] | clutch travel checking tool | (-).0216 - H | (-).0216 - H
[1i] | hydraulic control transmitter removal tool | (-).0216 - J | (-).0216 - J
[1j] | hydraulic control clutch stop clipping tool | (-).0216 - K | (-).0216 - K
[1k] | double flywheel refitting tool (x2) | (-).0216 - L | 9040 - T
[1l] | gear lever locking tool | (-).0216 - M | (-).0216 - M