E--B19V1 - 206

GENERAL REPAIR TIME SCHEDULE PRESENTATION

The operation times shown in this schedule are invoicing times expressed in hours and hundredths of an hour ; These times correspond to operations carried out in accordance with the requirements of the technical documentation, on vehicles normally maintained by the peugeot dealerships PEUGEOT, using original replacement parts .

Any operation name finishing with the letter A comprises all the operations of removal/refitting, cleaning, replacement etc. and the adjustments necessary for these operations to be carried out on a standard production vehicle .

For bodywork operations, these are incorporated in removal/refitting of detachable components ; This definition corresponds to all threaded, clipped or bonded parts, the removal of which is essential for the bodywork operation to be carried out ; The overall time can be broken down into 4 tasks, identified by the letters M -T - S - E allowing any invoicing to be carried out at different labour rates .

Certain work is given a designation without a repair schedule time (e.g. straightening); invoicing is for the time spent, rounded up to the next tenth of an hour .

The road test or bench test time is not included in the operation times, with the exception of regular maintenance .

1 - SETTING UP A REPAIR TIME SCHEDULE OPERATION

|  | constituent processes | example
--- | --- | --- | ---
principal operation |  |  | 01001A - removal - refitting power unit 7,60
| including | operation already included in the principal operation this operation is entirely separate. it is in the schedule and may itself comprise various processes | 13003A - removal - refitting power unit 14008A -removal - refitting air cleaner
| supplement | operation concerning additional equipment the time is added to the time for the principal operation for purposes of invoicing | 01001K - models with air conditioning and power steering 1,20 01001L - models with power steering 0,60 01001M - models with air conditioning 0,70
| additional | operation that can be carried out in addition to the principal operation, as removal operations have already been carried out the time is added to the time for the principal operation for purposes of invoicing | 01001N - clutch overhaul 0,30

2 - PROCESSES INCLUDED, ADDITIONS AND SUPPLEMENTS

The overall time for the principal operation is not the sum of the times for the processes included, with additions or supplements carried out separately .

Certain stages of various operations may be common and are counted only once for the purpose of timing .

Example :

- operation 1 -replacement of front brake pads 0,80 h
- operation 2 -replacement of one front brake caliper 1,20 h ; additional : replacement of front brake pads 0,40 h ; total for the operation 2 : 1,60 h

These 2 operations have common stages; supply of the vehicle, removal/refitting of wheels, etc. .

Consequently : The time for replacement of the pads, carried out as in addition to the replacement of a brake caliper, is less than the replacement time for brake pads when this operation is carried out on its own, because the common stages already included in the replacement of the caliper are not counted for .

Therefore one cannot add together operation 1 and operation 2, which would give 2,00 h instead of 1,60 h .

3 - TASKS

The various tasks are indicated by a letter followed by a three star letter stating the technical level of the operation :

- M - mechanical
- T - panel work
- S - trim
- E - electrical
- P - paint

4 - NUMBERING OF OPERATIONS

example
group | sub-group | serial number | letter | description | parts catalogue page (*)
--- | --- | --- | --- | --- | ---
0 | 1 | 004 | A | engine replacement | 02A 75A-3
(*) this information is optional

Group : 0 to 9 .

Sub-group : 0 to 9 .

The code for the first two characters of the operation number is identical to the code used for part numbers; see section : numbering of groups and sub-groups .

Serial number : Sequence without any specific meaning .

Letter :

- A - principal operation
- B to T and Y (not O) - additional or extra operation specific to the nominal operation of the same number
- R - straightening or repairing operation
- U - class 1 painting
- V - class 2 painting
- W - class 3 painting
- X - anti-chip operation
- Z - class 0 painting

examples
numbering of operations | description | tasks | time
--- | --- | --- | ---
01.004A | engine replacement (including) 01.002A removal/refitting engine 01.002L engine stripping/retrimming | M* | 11,30
01.004M 01.004E | models with air conditioning lpg version (supplement) | M* | 0,40 2,10
01.004F | removal/refitting of the under-engine protection (additional) | M* | 0,10
72.120A | partial replacement of the rear floor | E* T* T** S* S** | 0,50 1,30 10,00 3,10 1,30

5 - MODEL CODE

3 characters (The letter defines the vehicle range) .

The list of model codes is shown at the top of each repair time schedule for each vehicle .