B2CG57K1 - 206 MA GEARBOX

DISMANTLING-ASSEMBLY GEARBOX CASING

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | differential bearing outer race fitting drift | (-).0317-AJ | (-).0317-AJ

2 - PRELIMINARY OPERATIONS

Dismantling : Gearbox .

Removal : Gearbox casing .

3 - DISMANTLING

Drift out the outer race (1) of the final drive left-hand bearing, using the notches in the casing .

4 - REASSEMBLING

Fit the new final drive left hand bearing outer race (1) using the tool [1] and a press .

5 - COMPLEMENTARY OPERATION(S)

WARNING : observe the cleaning and refitting conditions .

Refitting : Gearbox casing .

Reassembling : Gearbox .