B2CG81K1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING VEHICLE SPEED SENSOR AUTOADAPTIVE AUTOMATIC GEARBOX (AL4)

1 - REMOVAL

NOTE : do not drain the gearbox .

Disconnect the battery + terminal .

Place the vehicle on a lift .

Disconnect the vehicle speed sensor connector (2) .

Remove :

- the bolt (1)
- vehicle speed sensor (2)

2 - REFITTING

Replace the sensor o ring (2) .

Fit :

- vehicle speed sensor (2)
- the bolt (1) : tightening torque 1 da.Nm

Reconnect the vehicle speed sensor connector (2) .

Reconnect the positive terminal of the battery .