C5BG00F1 - 206

REMOVAL - REFITTING FUEL CAP COVER

1 - REMOVAL

Remove the fuel cap .

Remove the key .

Fit a protector under the cover (1) .

Press and turn (opposite direction to the arrow) the cap (2) to detach it from the lugs (A) of the cover .

Remove the cover (1) .

2 - REFITTING

Fit opposite the arrow, the lug cut at right angles (B) .

Engage all three lugs by turning (in the direction of the arrow) and press .

Refit the fuel cap .