C4CG27F1 - 206 CABRIOLET

REMOVAL - REFITTING : REAR QUARTER PANEL WEATHERSTRIP END PIECE

1 - REMOVAL

Place the vehicle in cabriolet position .

REMOVE THE REAR QUARTER PANEL UPPER SEAL .

Move aside the front upper section of the trim panel (1) .

Loosen the door aperture seal (2) at the rear .

Remove :

- the clips (3)
- the weatherstrip end piece (4) upwards

2 - REFITTING

NOTE : apply a product to assist fitting on the flange (example: soapy water) .

Engage the centring pin (5) in the opening (A) .

Position the weatherstrip end piece by engaging the flange (B) in the seal at (C) .

Fit new clips (3) .

Continue the fitting operations in the reverse order to removal .