C4BG0WF1 - 206 CABRIOLET

REMOVAL - REFITTING MOVING REAR SHELF

1 - REMOVAL

NOTE : change the vehicle into the coupé version .

Open the luggage compartment .

APPLY THE OPERATING PROCEDURE FOR HYDRAULIC PUMP LOAD REDUCTION .

REMOVE DETACHABLE SHELF PROTECTOR .

Remove the fasteners (1) .

OPEN THE ROOF MANUALLY .

Fold down the metal hingeing mechanism (2) .

Detach then remove the detachable shelf (3) .

2 - REFITTING

Proceed in the reverse order to removal .

Tighten the bolt (1) to 0.9 da.Nm .

Test operation .