C4CG1AF1 - 206

REMOVAL - REFITTING FRONT DOOR TRIM PANEL

1 - SPECIAL TOOLS

[1] Trim pliers (-).1311 .

2 - REMOVAL

Open the door .

Lower the glass fully .

Remove :

- the window winder (1) (according to specification)
- the fastener (2)
- the recessed gripper (3)
- the interior handle finisher (4)
- the interior cheater (5)
- the bolts (6) - (7)
- the door trim (8) (using the tool [1])

3 - REFITTING

Proceed in the reverse order to removal .