B2CB0DK1 - 206 AL4 AUTOMATIC GEARBOX

IDENTIFICATION AUTOMATIC GEARBOX

1 - IDENTIFICATION

The automatic gearbox is identified by a self-adhesive label (A) or an engraving (B) :

- (1) unit reference
- (2) serial number

2 - TIGHTENING TORQUES

reference | da.Nm
--- | ---
special features | without
(1) pre-tightening : converter | 1.0
(1) tightening : converter | 3.0
(2) gearbox mounting on crankcase | 5.2
(3) speedometer drive | 1.0
(4) solenoid valves and/or regulators on hydraulic block | 0.9
(5) hydraulic block | 0.8
(6) hydraulic block housing | 0.8
(7) automatic gearbox input speed sensor | 1.0
(8) automatic gearbox output speed sensor | 1.0
(9) supply pressure sensor | 0.9
(10) flow control solenoid in the exchanger | 1.0
(11) multi-function switch | 1.0
(12) cover stop | 1.5
(13) automatic gearbox heat exchanger | 5.0
(14) filler plug | 2.4
(15) level plug | 2.4
(16) gearbox drain plug | 3.3
(17) gearbox bracket | 4.5
drive shaft nut (M24 X 150) | 32.5