B2CT0LK1 - 206 AL4 AUTOMATIC GEARBOX

MODIFICATION OIL CAPACITY

1 - MODIFICATION(S) TO THE RANGE : DRAIN / REFILL / CHECK OIL LEVEL

Modify the following brochures :

- 206 autoadaptive automatic gearbox : brochure 1332
- 306 autoadaptive automatic gearbox : brochure 1306 - 1380
- 406 autoadaptive automatic gearbox : brochure 1221 - 1384 - 1417

The values for the quantity of oil for work on the autoactive automatic gearbox AL4 or on its components have changed .

2 - QUANTITY OF OIL TO USE

2 - 1 - AFTER REMOVAL/REFITTING OF HYDRAULIC BLOCK HOUSING

Old value : 0.5 litre(s) .

New value : 1.5 litre(s) .

2 - 2 - AFTER DRAINING AND REPLACEMENT OF HYDRAULIC BLOCK

Old value : 3.5 litre(s) .

New value : 4.5 litre(s) .

2 - 3 - AFTER DRAINING AND REPLACEMENT OF CONVERTER

Old value : 4.5 litre(s) .

New value : 5 litre(s) .