D5AG0AF1 - 206 CABRIOLET

REMOVAL - REFITTING REAR QUARTER PANEL SPEAKER

1 - REMOVAL

Remove :

- THE REAR SEAT
- THE REAR SEAT BACK REST
- THE REAR QUARTER PANEL SIDE TOP TRIM
- REMOVE THE REAR QUARTER PANEL SIDE TOP TRIM

Remove the speaker fittings (1) .

Release the speaker (2) .

Disconnect the speaker connector (3) .

Remove the loudspeaker (2) .

2 - REFITTING

Proceed in the reverse order to removal .

Test operation .