C4EB1NF1 - 206 5 ESTATE

IDENTIFICATION : REMOVABLE PARTS

1 - TAILGATE

reference | description | Part No. | thickness (mm) | comment(s)
--- | --- | --- | --- | ---
1 | tailgate assembly | yes |  | 2 to 11
2 | tailgate | yes | 0,72 |
3 | tailgate inner panel | no | 0,67 |
4 | right tailgate hinge stiffener | no | 1,47 |
5 | left tailgate hinge stiffener | no | 1,47 |
6 | tailgate strut support | no | 1,17 |
7 | left tailgate inner panel stiffener | no | 1,47 |
8 | left tailgate inner panel stiffener | no | 1,47 |
9 | tailgate lock fixing stiffener | no | 1,47 |
10 | rear window lock stiffener | no | 1,17 |
11 | tailgate window lock support | no | 0,47 |
12 | right tailgate hinge | yes |  |
13 | left tailgate hinge | yes |  |

2 - REAR DOOR

reference | description | Part No. | thickness (mm) | comment(s)
--- | --- | --- | --- | ---
| rear left door assembly | yes |  | 1 to 12
1 | rear left door inner panel | no | 0,67 |
2 | rear door inner panel stiffener | no | 1,17 |
3 | rear left door side impact stiffener rear support | no | 1,17 |
4 | rear left door side impact stiffener | no | 0,67 |
5 | rear left door slide frame | no | 0,67 |
6 | rear left door slide frame rear support | no | 1,17 |
7 | tapped plate | no | 6 |
8 | tapped plate | no | 6 |
9 | rear left door upper hinge stiffener | no | 1,17 |
10 | rear door lower hinge stiffener | no | 1,47 |
11 | rear left-hand door | yes | 0,72 | 11+12
12 | rear left door horizontal stiffener | no | 0,67 |